Results of MCP3202demojcfbreak.spin

Nstep: 0

SWITCH Base method

PHOVER Calls hover method, no signal

Nstep: 2

SWITCH Back to base method

PCHECKTUNE Calls another method

Total Time= 451728

a: 1567 Meas 100 samples of fwd signal, and avg

b: 1360 Meas 100 samples of Ref signal, and avg

Nstep: 3

SWITCH Back to base method

PCHKBAND Calls another method

Total Time= 451728

a: 1586 Meas 100 samples of fwd signal, and avg

b: 1393 Meas 100 samples of Ref signal, and avg

Nstep: 4

SWITCH Back to base method

PCHKBAND

Nstep: 0

SWITCH

PHOVER No signal

Total Time= 451728

a: 329 Measuring 100 samples of noise on fwd

b: 184 Measuring 100 samples of noise on fwd

Nstep: 1

SWITCH

PCALCSWR

Total Time= 451728

a: 330

b: 184

Nstep: 2